======== STARTING =========
>>>> [LIBDMTCP loaded successfully.] <<<<
>>>> [dmtcp library is loaded and running.] <<<<
>>>> [Loaded with dmtcp_launch; checkpoint and restart are available.] <<<<
>>>> [Launching runenergyplus in /home/atizawa/5ZoneTsetTest/tmpJRgBZ1] <<<<
>>>> [waiting for connection from Energy Plus on port 45208] <<<<

=============== EnergyPlus =================
   Input file  : SmallOffice2004TsetTest_V720.idf
   Weather file: USA_HI_Honolulu.911820_TMY2.epw
ExpandObjects Started.
No expanded file generated.
ExpandObjects Finished. Time:     0.044

=============== EnergyPlus =================
   Input file  : SmallOffice2004TsetTest_V720.idf
 Missing Energy+.ini
 EnergyPlus Starting
 EnergyPlus-Linux-OMP-64 7.2.0.006, YMD=2015.09.24 12:34
 Processing Data Dictionary
 Processing Input File
 Initializing Response Factors
 Calculating CTFs for "MASS NON-RES EXT WALL", Construction #1
 Calculating CTFs for "MASS NON-RES EXT WALL", Construction #1
 Calculating CTFs for "ATTIC NON-RES FLOOR", Construction #2
 Calculating CTFs for "ATTIC NON-RES FLOOR", Construction #2
 Calculating CTFs for "ATTIC NON-RES ROOF", Construction #3
 Calculating CTFs for "EXT-SLAB", Construction #4
 Calculating CTFs for "INT-WALLS", Construction #5
 Calculating CTFs for "DROPCEILING", Construction #7
 Calculating CTFs for "INTERIORFURNISHINGS", Construction #9
 Initializing Window Optical Properties
 Initializing Solar Calculations
 Allocate Solar Module Arrays
 Initializing Zone Report Variables
 Initializing Surface Report Variables
 Determining Shadowing Combinations
 Computing Window Shade Absorption Factors
 Proceeding with Initializing Solar Calculations
 Initializing Surfaces
 Initializing Outdoor environment for Surfaces
 Initializing Temperature and Flux Histories
 Initializing Window Shading
 Computing Interior Absorption Factors
 Computing Interior Diffuse Solar Absorption Factors
 Computing Interior Diffuse Solar Exchange through Interzone Windows
 Initializing Solar Heat Gains
 Initializing Internal Heat Gains
 Initializing Interior Solar Distribution
 Initializing Interior Convection Coefficients
 Gathering Information for Predefined Reporting
 Completed Initializing Surface Heat Balance
 Calculate Outside Surface Heat Balance
 Calculate Inside Surface Heat Balance
 Calculate Air Heat Balance
 Initializing HVAC
 Warming up
 Warming up
 Warming up
 Warming up
 Warming up
 Warming up
 Performing Zone Sizing Simulation
 Warming up
 Warming up
 Warming up
 Warming up
 Warming up
 Warming up
 Performing Zone Sizing Simulation
 Calculating System sizing
 Calculating System sizing
 Initializing Simulation
 Reporting Surfaces
 Initializing New Environment Parameters
 Warming up {1}
 Instantiating Building Controls Virtual Test Bed
 ExternalInterface initializes.
>>>> [connecting to master controller at localhost:40082] <<<<
>>>> [connected to master: master_addr=('localhost', 40082), local_addr=('127.0.0.1', 59494)] <<<<
>>>> [waiting for data from Energy Plus] <<<<
 Number of outputs in ExternalInterface = 7
 Number of inputs  in ExternalInterface = 3
 Warming up {2}
 Warming up {3}
 Warming up {4}
 Warming up {5}
 Warming up {6}
 Starting Simulation at 01/21 for HONOLULU ANN HTG 99% CONDNS DB
 Initializing New Environment Parameters
 Warming up {1}
 Warming up {2}
 Warming up {3}
 Warming up {4}
 Warming up {5}
 Warming up {6}
 Starting Simulation at 08/21 for HONOLULU ANN CLG .4% CONDNS WB=>MDB
 Initializing New Environment Parameters
 Warming up {1}
 Warming up {2}
 Warming up {3}
 Warming up {4}
 Warming up {5}
 Warming up {6}
 Starting Simulation at 06/21 for HONOLULU HI USA TMY2-22521 WMO#=911820
 ExternalInterface starts first data exchange.
>>>> [Data from master controller: checkpoint
] <<<<
>>>> [checkpoint requested.] <<<<
>>>> [closing socket to master controller.] <<<<
>>>> [creating checkpoint.] <<<<
>>>> [just finished checkpoint or restore.] <<<<
>>>> [checkpoint or restart completed; re-connecting to master controller.] <<<<
>>>> [connecting to master: local_addr=('127.0.0.1', 59494), master_addr=('localhost', 40082)] <<<<
>>>> [reconnected to master controller.] <<<<
>>>> [Data from master controller: 2 0 3 0 0 0.000000000000000e+00 1.730463697828669e+01 1.730463697828669e+01 1.000000000000000e+00 
] <<<<
>>>> [Data from master controller: ] <<<<
>>>> [Socket shutdown by master controller; shutting down connection to Energy Plus.] <<<<
>>>> [shutting down energy plus socket.] <<<<
>>>> [Socket shutdown by Energy Plus; shutting down connection to master controller.] <<<<
>>>> [shutting down master socket.] <<<<
>>>> [received error message during shutdown of master socket.] <<<<
>>>> [[Errno 9] Bad file descriptor] <<<<
Error: The server closed the socket while the client was reading.
 **FATAL:Error in ExternalInterface: Check EnergyPlus *.err file.
 EnergyPlus Run Time=00hr 01min  1.75sec
EnergyPlus Terminated--Error(s) Detected.
 ReadVarsESO program starting.
 EOF encountered on eplusout.eso while reading data
 probable EnergyPlus error condition -- check eplusout.err
 ReadVarsESO program terminated.
 ReadVars Run Time=00hr 00min  0.08sec
 ReadVarsESO program starting.
 EOF encountered on eplusout.eso while reading data
 probable EnergyPlus error condition -- check eplusout.err
 ReadVarsESO program terminated.
 ReadVars Run Time=00hr 00min  0.00sec
  Started HVAC Diagram
  Complete

EnergyPlus output files are located in: "/home/atizawa/5ZoneTsetTest/tmpJRgBZ1/Output"


===== EnergyPlus terminated with error =====

>>>> [Energy Plus completed with an error. Temporary directory '/home/atizawa/5ZoneTsetTest/tmpJRgBZ1' has been retained.] <<<<
>>>> [./ep_worker complete.] <<<<
