**Highlights**

* Effect of duration in heat-driven processes on system performance is studied
* Optimum parameters for different indicators are same
* Optimal inter-stage pressure is sensitive to conditions for two-stage cycle
* Optimal inter-stage temperature varies less for layout with cascade condenser
* Performance of layout with cascade subcooler is fixed on intermediate temperature