**Author information：**

Qian Zhou, College of Marine Science and Technology, Zhejiang Ocean University, Zhoushan 316022, China; zhouqian@zjou.edu.cn;

Feng Gui, College of Marine Science and Technology, Zhejiang Ocean University, Zhoushan 316022, China; fgui@zjou.edu.cn;

Benxuan Zhao, Zhejiang Zhonglan Environmental Technology Co. Ltd; Wenzhou, 325000, China; zbx515@163.com;

Jingyi Liu, National Engineering Research Center for Marine Aquaculture, Zhejiang Ocean University, Zhoushan 316022, China; liujingyi@zjou.edu.cn;

Huiwen Cai, College of Marine Science and Technology, Zhejiang Ocean University, Zhoushan 316022, China; caihuiwen@zjou.edu.cn;

Kaida Xu, Zhejiang Province Key Laboratory of Mariculture and Enhancement, Zhejiang Marine Fisheries Research Institute, Zhoushan 316022, China; h01011@zjou.edu.cn;

Sheng Zhao, Correspondence, College of Marine Science and Technology, Zhejiang Ocean University, Zhoushan 316022, China; zhaosh@zjou.edu.cn.

**Funding:**

This study is sponsored by the National Key R&D Program of China (No. 2019YFD0901204);

the Fundamental Research Funds for Zhejiang Provincial Universities and Research Institutes (No.2021JD006); and the Key R&D Program of Zhejiang Province (No. 2019C02056).