グラフ, 棒グラフ

自動的に生成された説明**Supplemental Fig.1** Variation of ammonia concentration in AlN or AlN/CNT composite filler as a function of time of atmospheric exposure (atmospheric exposure conditions: Temperature: 24.3oC, Humidity: 75%)